AADS Utility Services

Service Manipulation:

svc utilserv start
svc utilserv stop
svc utilserv restart

Config URL: https://IP_Utility_Server:8543/admin.html

Enable Port 80

cdto misc
sudo ./us-http-port.sh --enable
sudo ./us-tls.sh --enable

TLS Port for Phones: 1543

1. SET GROUP ID on AADS for Phone Type.
2. Goto /var/www/html
3. . In the upgrade file, replace the GET 46xxsettings.txt entry with GET / 46xxsettings.txt, where is the group identifier assigned to the phone model.
For example, if you assigned 123 to the 96×1 phone model, the updated entry must look as follows: GET 123/46xxsettings.txt.